Instruction for production :

Tolerance : ISO 2768-Fine

Support\_Sensor\_V2 : Quantity 50

- Material : PVC Black

- No Thread

Bride\_6\_Pouce\_Metal : Quantity 12 or 24 (quote both please)

- Material : POM Black

- 24 M8 Threads (12 blind)

- 4 M4 Threads (blind)

Bras Hydro : Quantity 30

- Material Stainless Steel 316

- 2 M5 Threads

- Tolerance is fine only for holes, and can be rough elsewhere.

Bras Pied : Quantity 20

- Material Stainless Steel 316

- No Thread

- Tolerance is fine only for holes, and can be rough elsewhere.

Bras Hydro Long : Quantity 10

- Material Stainless Steel 316

- 2 M5 Threads

- Tolerance is fine only for holes, and can be rough elsewhere.

IA60\_Moule : Quantity 2

- Material : Aluminium - Sand Blasted

- 1 M5 Threads

IA200\_Moule : Quantity 2

- Material : Aluminium - Sand Blasted

- 1 M5 Threads

IA60\_Support\_Piezo : Quantity 100

* Material : PVC Black

IA200\_Support\_Piezo : Quantity 100

* Material : PVC Black

IA60\_Disque\_Superieur : Quantity 200

- Material : PVC black

IA200\_Corps : Quantity 100

- Material : PVC black

IA200\_Corps : Quantity 100

- Material : Stainless Steel 316