Instruction for production :

Tolerance : ISO 2768-Fine

Corps\_AL\_V2 : Quantity 50 / 100 (quote both please)  
 - Material : PVC black or grey

Disque\_Superieur : Quantity 50 / 100 (quote both please)

- Material : PVC

Support\_Capteur : Quantity 50 / 100 (quote both please)

- Material : PVC

Moule : Quantity 10

* Material : Aluminium
* Finish : None / Sand blasted (quote both please)
* 3 Threads in M4

Protection : Quantity 50 / 100 (quote both please)

* Material Stainless Steel 316
* Can be welded
* Except for the 2 holes, tolerance is rough

Mise\_Air\_Libre : Quantity 50

* Material Stainless Steel 316
* M7-0.75 (fine) Tapping at the bottom (inside, diameter 6.2mm, length 10mm)
* M10-1.5 (normal) Thread at the bottom (outside, diameter 10mm, length 18.2mm)
* M14-1 (fine) Tapping in the top hole (inside, diameter 13mm, length 7mm)

Bouchon : Quantity 50