Instruction for production :

Tolerance : ISO 2768-Fine

Bras lateral : Quantity 24 / 48 (quote both please)  
 - Material : Stainless Steel 316

* Tolerance is fine only for holes, and can be rough elsewhere.

Bride\_6\_Pouce\_Metal : Quantity 12 or 24 (quote both please)

- Material : Stainless Steel 316

- 24 M8 Threads (12 blind)

- 4 M4 Threads (blind)

Support\_Sensor : Quantity 24 / 48 (quote both please)

- Material : PVC

Finish is normal, no need to sand them.