Instruction for production :

Tolerance : ISO 2768-Fine

Corps\_AL\_V2 : Quantity 50 / 100 (quote both please)  
 - Material : PVC black or grey

Disque\_Superieur : Quantity 50 / 100 (quote both please)

- Material : PVC

Support\_Capteur : Quantity 50 / 100 (quote both please)

- Material : PVC

Moule : Quantity 10

* Material : Aluminium
* Finish : None / Sand blasted (quote both please)
* 3 Threads in M4

Protection : Quantity 50 / 100 (quote both please)

* Material Stainless Steel 316
* Can be welded
* Except for the 2 holes, tolerance is rough